|  |  |
| --- | --- |
| 2022 Water Grant Program | CEC Plumbing Fixtures Requirements – focus is on Noncompliant Fixture as defined |
| Replacement of toilets using more than 1.6 gallons per flush  | Any toilet manufactured to use more than 1.6 gallons of water per flush. |
| Installation of waterless urinals and low flow urinals  | Any urinal manufactured to use more than 1 gallon of water per flush. |
| Replacement of low flow showerheads with a flow rate greater than 1.8 gallons per minute   | Any showerhead manufactured to have a flow capacity of more than 2.5 gallons of water per minute.  |
| Installation Installing motion sensor-activated faucets, water efficient faucets and faucet aerators  |  Any interior faucet that emits more than 2.2 gallons of water per minute.  |