APPROVED BY THE CALIFORNIA BUILDING STANDARDS COMMISSION JUNE 27, 2023

# COMMISSION ACTION MATRIX Building fire and other – STRUCTURAL DESIGN/LATERAL FORCES AD-HOC (BFO/SDLF) CODE ADVISORY COMMITTEE

## 2022 california BUILDING code, TITLE 24, PART 2 AGENCY: division of the state architect, DSA-SS/CC 03/22

### LEGEND:

**CAC Actions:** Approve, Disapprove, Approve as Amended, Further Study Required

**Agency Responses:** Accept, Disagree, Withdraw

**CBSC Actions:** Approve, Disapprove, Approve as Amended, Further Study Required

**Matrix Paper Color** (for commission action only): GREEN = uncontested items, YELLOW = challenged items, SALMON = withdrawn, no action required

If using assistive technology, please adjust your settings to recognize underline, strikeout, italic and ellipsis.

* Model Code language appears upright
* Existing California amendments appear in *italic*
* Amended model code or new California amendments appear *underlined & italic*
* Repealed model code language appears ~~upright and in strikeout~~
* Repealed California amendments appear in *~~italic and strikeout~~*
* Ellipses (...) indicate existing text remains unchanged

### Chapter 2, Definitions

Amend Definition of EQUIPMENT

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item Number 1** | **Code Section** | **CAC Action** | **Agency Response** | **Public Comments** | **Annotations** | **CBSC Action** |
| DSA-SS/CC 03/22-1-1 | ***(6) MOVABLE EQUIPMENT*** | **Further Study** | **Disagree** | No public comments received. | Add the word “fixed” to the definition and make an editorial change.  **Code Advisory Committee (CAC): FS under Criteria #5, 6.** Recommended to consider removing the proposed word “fixed” and adding other qualifying language such as “equipped with removable anchors” to clarify the intent.  **See ISOR for detailed response to recommendation.** | **Approve** |

### Chapter 17A, special inspections and tests

Amend Section 1703A.1.1

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item Number 2** | **Code Section** | **CAC Action** | **Agency Response** | **Public Comments** | **Annotations** | **CBSC Action** |
| DSA-SS/CC 03/22-2-1 | **1703*A*.1.1 Independence.** | **Further Study** | **Accept** | No public comments received. | Add language to existing section to clarify the distinction between the inspections performed by special inspectors employed by an approved agency and the project inspector of record (IOR) or the entity providing inspection services.  **CAC: FS under Criteria #6.** Recommended to consider replacing “or” with “and” and adding “broker” to the entities listed in the proposed language to clarify the intent.  **See ISOR for detailed response to recommendation.** | **Approve** |

### Chapter 19*A*, concrete

Amend Sections 1905A.1.9

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item Number 3** | **Code Section** | **CAC Action** | **Agency Response** | **Public Comments** | **Annotations** | **CBSC Action** |
| DSA-SS/CC 03/22-3-1 | **1905*A.*1.*9* ACI 318, Section 18.5.** | **Approve** | **Disagree** | No public comments received. | Amend to correct the referenced section and formatting issues.  **Code Advisory Committee (CAC)** requested DSA to consider refining the proposal language in order to clarify the intent of the modification to ACI 318 Section 18.5.2.1. DSA modified the proposed language to include CAC suggestions.  **See ISOR for detailed response to recommendation.** | **Approve** |

### Chapter 21, masonry

Amend Section 2115.7

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item Number 4** | **Code Section** | **CAC Action** | **Agency Response** | **Public Comments** | **Annotations** | **CBSC Action** |
| DSA-SS/CC 03/22-4-1 | ***2115.7 Compressive strength*** | **Approve** | **Accept** | No public comments received. | Add language to existing section to clarify a minimum compressive strength for concrete and clay masonry. | **Approve** |

### CHAPTER 21*A*, MASONRY

Amend Sections 2104A.1.3.1 Article 3.2 F, 2104A.1.3.11.1, 2104A.2, 2107A.6, 2108A.4

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item Number 5** | **Code Section** | **CAC Action** | **Agency Response** | **Public Comments** | **Annotations** | **CBSC Action** |
| DSA-SS/CC 03/22-5-1 | ***2104A.1.3.1 TMS 602, Article 3.2 F Cleanouts.*** | **Approve** | **Accept** | No public comments received. | Add language to existing section to clarify intend. | **Approve** |
| DSA-SS/CC 03/22-5-2 | ***2104A.1.3.11.1 TMS 602, Article 2.3 A & 2.3 B Masonry unit materials.*** | **Approve** | **Accept** | No public comments received. | Add the word “reinforced” to #1 to clarify intend. | **Approve** |
| DSA-SS/CC 03/22-5-3 | ***2105A.2 Compressive strength*** | **Approve** | **Accept** | No public comments received. | Add language to existing section to clarify a minimum compressive strength for concrete and clay masonry. | **Approve** |
| DSA-SS/CC 03/22-5-4 | ***2107A.6 Masonry Compressive Strength.*** | **Approve** | **Accept** | No public comments received. | Repeal language from existing section to clarify requirements for minimum compressive strength. | **Approve** |
| DSA-SS/CC 03/22-5-5 | ***2108A.4 TMS 402, Section 9.1.9.1.1.*** | **Approve** | **Accept** | No public comments received. | Repeal language from existing section to clarify requirements for minimum compressive strength. | **Approve** |

### Chapter 23, wood

Amend Section 2301.1.4

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item Number 6** | **Code Section** | **CAC Action** | **Agency Response** | **Public Comments** | **Annotations** | **CBSC Action** |
| DSA-SS/CC 03/22-6-1 | ***2301.1.4 Prohibition.*** | **Further Study** | **Accept** | No public comments received. | Add #9 to prohibitions for DSA regarding cross-laminated timber.  **CAC: FS under Criteria #6.** Recommended to reconsider if the amendment is necessary, coordinate with OSHPD and update numbering as necessary.  **See ISOR for detailed response to recommendation.** | **Approve** |