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FINAL EXPRESS TERMS 
ITEM 1-1
Chapter 2, Definitions, Section 202 Educational Entity in Receipt of Financial Assistance
EDUCATIONAL ENTITY IN RECEIPT OF FINANCIAL ASSISTANCE. Any college, university, or other postsecondary institution, or a public system of higher education, or a K-12 educational entity; system of career and technical education, or other school system; or any corporation, partnership, or other private organization including a sole proprietorship which is principally engaged in the business of providing education, any part of which is a covered entity that is a recipient of state support or federal financial assistance including, but not limited to, federal Pell Grants or work-study programs. See  California Code of Regulations Title 2, Division 4.1, Chapter 5, Subchapter 9, Article 2, Section 14020.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 1-2
Chapter 2 Definitions, Section 202 Housing at a Place of Education
HOUSING AT A PLACE OF EDUCATION. Housing operated by or on behalf of an elementary, secondary, undergraduate or postgraduate school, or other place of education, including dormitories, suites, apartments or other places of residence. See also PUBLIC HOUSING and PLACE OF PUBLIC ACCOMMODATION.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 2-1
Chapter 2 Definitions, Section 202 Place of Public Accommodation
PLACE OF PUBLIC ACCOMMODATION.  A facility operated by a private entity whose operations affect commerce and fall within at least one of the following categories:
(1) Place of lodging, …
(2) A restaurant, bar or …
(3) A motion picture house …
(4) An auditorium, convention center …
(5) A bakery, grocery store, …
(6) A laundromat, dry-cleaner, bank, barber shop, …
(7) A terminal, depot or …
(8) A museum, library, gallery or …
(9) A park, zoo, amusement park or …
(10) A nursery, elementary, secondary, undergraduate or post graduate private school, or other place of education;, including housing facilities provided for students or employees;
(11) A day-care center, senior citizen center, …
(12) A gymnasium, health spa …
(13) A religious facility;
(14) An office building; and
(15) A public curb or sidewalk.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 3-1
Chapter 2 Definitions, Section 202 Public Housing
PUBLIC HOUSING. [DSA-AC] Housing facilities constructed or altered by, for, or on behalf of a public entity, or constructed or altered as part of a public entity’s program to provide housing pursuant to United States Code of Federal Regulations, 28 CFR Part 35, Section 35.102(a), and California Code of Regulations Title 2, Division 4.1, Chapter 5, Subchapter 9, Article 1, Section 14000 and Article 2, Section 14020, including but not limited to the following:

1. …
2. …
3. Homeless shelters, group homes, halfway houses and similar social service center establishments;
4. …
Notation: 
Authority: Government Code Section 4450 
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 3-2
Chapter 2 Definitions, Section 202 Public Housing
1. …
2. …
3. (See ITEM 3-1)
4. Transient lodging, such as hotels, motels, hostels and other facilities providing accommodations of a short-term nature of not more than 30 days duration; 
5. … (See ITEM 3-4)
Notation: 
Authority: Government Code Section 4450 
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 3-3
Chapter 2 Definitions, Section 202 Public Housing
1. … 
2. …
3. (See ITEM 3-1)
4. Employer-provided housing for an employee or an employee and their family members, either temporary or permanent, such as fire station dormitories.
5. … (See ITEM 3-4)
Notation: 
Authority: Government Code Section 4450 
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 3-4
Chapter 2 Definitions, Section 202 Public Housing
1. … 
2. …
3. (See ITEM 3-1)
4. (See ITEMS 3-2 and 3-3)
5. Housing at a place of education, such as housing on or serving a public school, public college, or public university., or private educational entity in receipt of financial assistance. See EDUCATIONAL ENTITY IN RECEIPT OF FINANCIAL ASSISTANCE. 
Note: A public entity’s program to provide housing may include but is not limited to: the allocation of local, state or federal financial assistance, Community Development Block Grants, Low Income Housing Tax Credits, the California Multifamily Housing Program, loan agreements and housing bonds. Examples that are not considered a public entity’s program to provide housing may include but are not limited to: density bonuses, the receipt of public funds for the installation of energy efficiency features, seismic strengthening, water conservation and fire safety features. For additional information see “Guide to Public Housing Regulated in Chapter 11B of the California Building Code” and the “California Access Compliance Advisory Reference Manual” available on the Division of the State Architect’s website.
Notation: 
Authority: Government Code Section 4450 
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 4-1
Withdrawn. See Item 15-1.
ITEM 4.1-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-106.5 Defined Terms.
11B-106.5 Defined Terms…
ACCESS AISLE
…
DRIVEWAY
EDUCATIONAL ENTITY IN RECEIPT OF FINANCIAL ASSISTANCE
…
Notation: 
Authority: Government Code 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 5-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-202.4 Path of Travel requirements in alterations, additions and structural repairs.
11B-202.4 Path of travel requirements in alterations, additions and structural repairs. …
Exceptions:
1. Residential dwelling units shall comply with Section 11B-233.3.4.2 not be required to comply with Section 11B-202.4. Additions or alterations to residential facilities shall comply with Section 11B-233. 
2. …
Notation: 
Authority: Government Code Section 4450 and 12955.1(c)
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 6-1
Withdrawn.

ITEM 7-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-205.1 General.
11B-205.1 General. Operable parts on accessible elements, accessible routes, and in accessible rooms and spaces shall comply with Section 11B-309.
	Exceptions:
1. …

9. In residential dwelling units with mobility features where receptacles are provided in a kitchen at a corner work surface, one receptacle shall be located 36 inches (915 mm) from either wall at the inside corner. 
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FIGURE 11B-205.1 Ex. 9
ELECTRICAL RECEPTACLES AT CORNER WORKSURFACES
Notation: 
Authority: Government Code Section 4450 and 12955.1(c) 
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 8-1, 8-2
Withdrawn. Similar item now proposed for Section 11B-233.2.1.  See Item 16.

ITEM 9-1
Withdrawn. Similar item now proposed for Section 11B-233.2.2.  See Item 16.

ITEM 10-1, 10-2
Withdrawn. The proposal is relocated to Section 11B-233.2.1. See Item 16.

ITEM 11
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-214 Washing machines and clothes dryers
11B-214 - WASHING MACHINES AND CLOTHES DRYERS
11B-214.1 General. …
SUB-ITEM 11-1
Section 11B-214.2 Washing machines.
11B-214.2 Washing machines. Where three or fewer washing machines are provided at least one shall comply with Section 11B-611. Where more than three washing machines are provided, at least two shall comply with Section 11B-611. 
Exception:  Public housing facilities required to comply with Section 11B-233.2 shall comply with Section 11B-233.2.4.
SUB-ITEM 11-2
Section 11B-214.3 Clothes dryers.
11B-214.3 Clothes dryers. Where three or fewer clothes dryers are provided, at least one shall comply with Section 11B-611. Where more than three clothes dryers are provided, at least two shall comply with Section 11B-611.
Exception:  Public housing facilities required to comply with Section 11B-233.2 shall comply with Section 11B-233.2.4.
Notation: 
Authority: Government Code Section 4450 and 12955.1(c)
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 12-1
Withdrawn. Similar item now proposed for Section 11B-233.2.3.  See Item 16.

ITEM 13-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-233.2.3 On-call rooms.
11B-223.2.3 On-call rooms. Where physician or staff on-call sleeping rooms are provided, at least 10 percent, but no fewer than one, of the on-call rooms shall provide mobility features complying with Sections 11B-806.2.3, 11B-806.2.4 and 11B-806.2.6. 11B-805.2.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 13.1-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-224
SECTION 11B-224 – TRANSIENT LODGING GUEST ROOMS, HOUSING
AT A PLACE OF EDUCATION AND SOCIAL CENTER ESTABLISHMENT
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 14-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Sections 11B-224.7 and 11B-233.4
11B-233.4224.7 Housing at a place of education. Housing at a place of education subject to this section shall comply with Sections 11B-224.1 through 11B-224.6 and 11B-806 for transient lodging guest rooms this section. For the purposes of the application of this section, the term “sleeping room” is interchangeable with “guest room” as used in the transient lodging standards.
11B-233.4.1 Housing at a place of education as public housing. Housing at a place of education as public housing shall comply with Sections 11B-233.2 and 11B-233.3. 
Exception: Housing facilities that are provided by or on behalf of a place of education, with residential dwelling units leased on a year-round basis exclusively to graduate students or faculty, and that do not contain any public use or common use areas available for educational programming, are not subject to Section 11B-224 and shall comply with Section 11B-233.
11B-233.4.2 Housing provided by an educational entity that is not an educational entity in receipt of financial assistance. Housing provided by an educational entity that is not in receipt of financial assistance shall comply with Section 11B-233.3. 
11B-233.4.3 Sleeping rooms with mobility and communications features.  In lieu of residential dwelling units complying with 11B-233.3.1.1, 11B-233.3.1.3 and 11B-233.3.5, facilities shall provide sleeping rooms complying with Sections 11B-224.1 through 11B-224.6, and Section 11B-806. For the purposes of the application of this section, the term “sleeping room” is interchangeable with “guest room” as used in the transient lodging standards.
Exception: Housing facilities that are provided by or on behalf of a place of education, with residential dwelling units leased on a year-round basis exclusively to graduate students or faculty, and that do not contain any public use or common use areas available for educational programming, are not subject to Section 11B-224 and shall comply with Section 11B-233.  11B-233.4.3.
11B-233.4.4224.7.1 Multibedroom housing units with mobility features. Multibedroom housing units containing accessible sleeping rooms with mobility features shall have an accessible route throughout the unit in compliance with Section 11B-809.2. Kitchens, when provided, within housing units containing accessible sleeping rooms with mobility features shall comply with Section 11B-804.
11B-224.7.2 Accessible dwelling units with adaptable features. Accessible dwelling units with adaptable features shall be provided as required by Section 11B-233.3.1.2. The number of required accessible dwelling units with adaptable features shall be reduced by the number of units with mobility features required by Section 11B-224.2.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 15-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Sections 11B-224.8 and 11B-233.5
11B-233.5224.8 Social service center establishments. Group homes, halfway houses, shelters or similar social service center establishments that provide either temporary sleeping accommodations or residential dwelling units subject to this section shall comply with Section 11B-233.3. as public housing shall comply with Sections 11B-233.2 and 11B-233.3. All other social service center establishments that provide either temporary sleeping accommodations or residential dwelling units shall comply with Section 11B-233.3.
11B-233.5.1224.8.1 More than 25-bed sleeping rooms. In sleeping rooms with more than 25 beds, a minimum of 5 percent of the beds shall have clear floor space complying with Section 11B-806.2.3.
11B-233.5.2224.8.2 More than 50-bed facilities. Facilities with more than 50 beds that provide common use bathing facilities shall provide at least one roll-in shower with a seat that complies with Section 11B-608. When separate shower facilities are provided for men and women, at least one roll-in shower shall be provided for each group.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 16-1.1 through 16-10.5
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-233 Residential Facilities
SECTION 11B-233—PUBLIC HOUSING RESIDENTIAL FACILITIES
11B-233.1 General. Public housing Residential facilities subject to this chapter with residential dwelling units shall comply with Section 11B-233.  See Chapter 2, Section 202 of this code for the definition of Public Housing and Place of Public Accommodation.
11B-233.2 Reserved. Public housing facilities.  Public housing facilities shall comply with Sections 11B-233.2 and 11B-233.3. 
Exceptions:  
1. Public housing facilities with 4 or fewer residential dwelling units shall not be required to comply with Section 11B-233.2.
2. Housing at a place of education as public housing containing either 4 or fewer sleeping rooms or 4 or fewer multi-bedroom housing units shall not be required to comply with 11B-233.2.
11B-233.2.1 Accessible routes.  Public housing facilities shall provide accessible routes as required by Section 11B-206. Section 11B-206.2.1 exception 2, the exception at Section 11B-206.2.2, and Section 11B-206.2.8 exceptions 2 and 3 shall not be permitted.
11B-233.2.2 Common Use Areas.  Public housing facilities permitted to use Section 11B-206.2.3, Exception 4 shall provide common use areas on the ground floor with amenities equal to those on upper floors.
11B-233.2.3 Fire alarm systems.  Public housing facilities are not permitted to use the exception at Section 11B-215.1.
11B-233.2.4 Washing Machines and Clothes Dryers.  Washing machines and clothes dryers provided in common use areas shall be front loading and shall comply with Section 11B-611.
11B-233.2.5 Additions.  Additions shall comply with Sections 11B-202.2, 11B-233.3.3 and this section.
11B-233.2.5.1 Entrances.  Where an addition to an existing building does not provide an entrance, at least one entrance in the existing building shall comply with Section 11B-206.4.
11B-233.2.5.2 Accessible route.  Where an addition to an existing building uses an existing entrance, at least one accessible route complying with Section 11B-206 shall be provided from site arrival points to the entrance, from the entrance to the addition, and shall connect all rooms, spaces and elements of the addition required to be accessible by this chapter.
11B-233.2.5.3 Toilet and bathing facilities.  Where a public or common use toilet facility is provided in the existing building but not in the addition, at least one toilet facility in the existing building shall comply with Section 11B-213 and shall provide an accessible route complying with Section 11B-206 from the toilet facility to the addition. Where a public or common use bathing facility is provided in the existing building but not in the addition, at least one bathing facility in the existing building shall comply with Section 11B-213 and shall provide an accessible route complying with Section 11B-206 from the bathing facility to the addition.
11B-233.2.5.4 Elements, spaces, and common use areas.  Where elements, spaces, or common use areas are provided in the existing building and equivalent elements, spaces or common use areas are not provided in the addition, at least one of each type of element, space, or common use area in the existing building shall be accessible in compliance with this chapter.
11B-233.2.6 Alterations. Alterations shall comply with Sections 11B-202.3, 11B-233.3.4 and this section.  
11B-233.2.6.1 Substantial alterations. A facility is substantially altered when the adjusted construction cost, as defined, of alterations to a facility containing 15 or more dwelling units, or 15 or more sleeping rooms in housing at a place of education, exceeds 75% of the replacement cost of the completed facility. 
11B-233.2.6.1.1 Residential dwelling units. Residential dwelling units complying with Sections 11B-233.3.1.1 and 11B-233.3.1.2 shall be provided in residential facilities, and sleeping rooms complying with Sections 11B-224.2 and 11B-224.4 shall be provided in housing at a place of education. See also Section 11B-233.4.
11B-233.2.6.1.2 Accessible Route.  At least one accessible route to each altered floor and altered area shall be provided and shall comply with Section 11B-206.
11B-233.2.6.1.3 Entrances.  At least one entrance in a building shall comply with Section 11B-404. 
11B-233.2.6.1.4 Toilet facilities.  Where common use toilet facilities are provided in substantially altered buildings, a minimum of one toilet facility shall comply with Section 11B-213. Where multiple floors with common use toilet facilities are substantially altered, each floor shall provide a toilet facility complying with Section 11B-213.
11B-233.2.6.1.5 Bathing facilities.  Where common use bathing facilities are provided in substantially altered buildings, a minimum of one common use bathing facility shall comply with Section 11B-213. Where multiple floors with common use bathing facilities are substantially altered, each floor shall provide a common use bathing facility complying with Section 11B-213.
11B-233.3 Public housing facilities. Facilities with residential dwelling units. Public housing facilities Facilities with residential dwelling units shall comply with Sections 11B-233.3 and 11B-809.
Note: Senior citizen housing may also be subject to Civil Code, Division 1. Part 2. Sections 51.2, 51.3 and 51.4.
11B-233.3.1 Minimum number: new construction. Newly constructed facilities with residential dwelling units shall comply with Section 11B-233.3.1. 
Exception: Where facilities contain 15 or fewer residential dwelling units, the requirements of Sections 11B-233.3.1.1 and 11B-233.3.1.3 shall apply to the total number of residential dwelling units that are constructed under a single contract, or are developed as a whole, whether or not located on a common site. 
11B-233.3.1.1 Residential dwelling units with mobility features. In facilities with residential dwelling units, at least 5 percent, but no fewer than one unit, of the total number of residential dwelling units shall provide mobility features complying with Sections 11B-809.1 through 11B-809.4 and shall be on an accessible route as required by Section 11B-206.
Exception: Housing at a place of education shall provide sleeping rooms complying with Section 11B-224.2 which shall be on an accessible route as required by Section 11B-206. See also Section 11B-233.4.
11B-233.3.1.2 Residential dwelling units with adaptable features. … [See Item 17-1 for proposed changes in Section 11B-233.3.1.2.6 Public housing facility site impracticality.]
11B-233.3.1.3 Residential dwelling units with communication features. In public housing facilities with residential dwelling units, at least 2 percent, but no fewer than one unit, of the total number of residential dwelling units shall provide communication features complying with Section 11B-809.5. 
Exception: Housing at a place of education shall provide sleeping rooms complying with Section 11B-224.4. See also Section 11B-233.4.
11B-233.3.2 Residential dwelling units for sale. ...
11B-233.3.3 Additions. …
11B-233.3.4 Alterations. …
11B-233.3.5 Dispersion. Residential dwelling units required to provide mobility features complying with Sections 11B-809.2 through 11B-809.4 and residential dwelling units required to provide communication features complying with Section 11B-809.5 shall be dispersed among the various types of residential dwelling units in the facility and shall provide choices of residential dwelling units comparable to, and integrated with, those available to other residents.
Exceptions:
1. Where multistory residential dwelling units are one of the types of residential dwelling units provided, one-story residential dwelling units shall be permitted as a substitute for multistory residential dwelling units where equivalent spaces and amenities are provided in the one-story residential dwelling unit. 
2. Housing at a place of education shall comply with Section 11B-224.5. See also Section 11B-233.4.
11B-233.3.6 Graduate student and faculty housing at a place of education. …
Notation: 
Authority: Government Code Sections 4450 and 12955.1(c)
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 17-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-233.3.1.2.6 Public housing facility site impracticality.
11B-233.3.1.2.6 Public housing facility site impracticality. The site impracticality tests in this section may be used to determine the number of required residential dwelling units with adaptable features in buildings without an elevator, located on sites with difficult terrain conditions or unusual characteristics.
Except as provided for in Section 11B-233.3.1.2.5, the provisions of this section do not apply to multistory dwelling units in non-elevator buildings.
11B-233.3.1.2.6.1 Single building with one common (lobby) entrance. The following may only be used for determining required access to multifamily dwelling units, in a single building with one common (lobby) entrance, located on a site with difficult terrain conditions or unusual characteristics:
All ground floor units in non-elevator buildings shall be adaptable and on an accessible route unless an accessible route to the common (lobby) entrance is not required as determined by Test No. 1, Individual Building Test, or Test No. 3, Unusual Characteristics Test, as described in this section.
Sites where either Test No. 1 or Test No. 3 is used and it is determined that an accessible route to the common (lobby) entrance is not required, a minimum of 20 percent of the ground floor dwelling units shall comply with Section 11B-809.6, and all remaining ground floor dwelling units shall comply with the features listed in Section 11B-233.3.1.2.6.5 unless exempted by Test No. 3, Unusual Characteristics Test. 
Test No. 1—Individual Building Test may only be used if the site has terrain over 15 percent slope.
Test No. 3—Unusual Characteristics Test may be used if applicable.
Provisions to Test Nos. 1 and 2. Where a building elevator is provided only as means of creating an accessible route to dwelling units on a ground floor, the building is not considered to be an elevator building for purposes of this code; hence, only the ground floor dwelling units would be covered.
11B-233.3.1.2.6.2 Test number one, individual building test. 
It is not required by this code to provide an accessible route when the terrain of the site is such that both of the following apply:
1. The slopes of the undisturbed site measured in a straight line between the planned entrance and all vehicular or pedestrian arrival points within 50 feet (15 240 mm) of the planned entrance exceed 15 percent; and
2. The slopes of the planned finished grade measured between the entrance and all vehicular or pedestrian arrival points within 50 feet (15 240 mm) of the planned entrance also exceed 15 percent.
If there are no vehicular or pedestrian arrival points within 50 feet (15 240 mm) of the planned entrance, the slope for the purposes of Test No. 1 will be measured to the closest vehicular or pedestrian arrival point.
For purposes of these requirements, vehicular or pedestrian site arrival points include public or resident parking areas, public transportation stops, passenger loading zones and public streets or sidewalks. To determine site impracticality, the slope would be measured at ground level from the point of the planned entrance on a straight line to: 
1. Each vehicular or pedestrian arrival point that is within 50 feet (15 240 mm) of the planned entrance, or
2. If there are no vehicular or pedestrian arrival points within the specified area, the vehicular or pedestrian arrival point closest to the planned entrance.
In the case of sidewalks, the closest point to the entrance will be where a public sidewalk entering the site intersects with the walk to the entrance. In the case of resident parking areas, the closest point to the planned entrance will be measured from the entry point to the parking area that is located closest to the planned entrance.
11B-233.3.1.2.6.3 Test number two, site analysis test.  
For a site having multiple buildings, or a site with a single building with multiple entrances, it is not required to provide a building entrance on an accessible route to all ground floor units under the following conditions:
1. Calculate the percentage of the total buildable area of the undisturbed site with a natural grade less than 10 percent slope. The analysis of the existing slope (before grading) shall be done on a topographic survey with 2 foot (610 mm) contour intervals with slope determination made between each successive interval. The accuracy of the slope analysis shall be certified by a licensed engineer, landscape architect, architect or surveyor.
2. Determine the requirement of providing an accessible route to planned multifamily dwellings based on the topography of the existing natural terrain. The minimum percentage of ground floor units required on an accessible route shall equal the percentage of the total buildable area (not restricted-use areas, flood plains or wetlands) of the undisturbed site with an existing natural grade of less than 10 percent slope.
3. In addition to the percentage established in paragraph (2), all ground floor units in a building, or ground floor units served by a particular entrance on an accessible route defined by a calculation of the straight line slope not exceeding 8.33 percent, between their planned entrances and an arrival point, shall be on an accessible route and comply with the provisions of Section 11B-809.6.
4. All additional ground floor units in a building, or ground floor units served by a particular entrance, not on an accessible route shall comply with the features listed in Section 11B-233.3.1.2.6.5.
5. In no case shall less than 20 percent of the ground floor dwelling units be on an accessible route and comply with the provisions of Sections 11B-809.6 through 11B-809.12.
11B-233.3.1.2.6.4 Test number three, unusual characteristics test. 
Unusual characteristics include sites located in a state or federally designated floodplain or coastal high-hazard areas and sites subject to other similar requirements of law or code that require the lowest floor or the lowest structural member of the lowest floor be designed to a specified level at or above the base flood elevation. An accessible route to a building entrance is impractical due to unusual characteristics of the site when:
1. The original site characteristics result in a difference in finished grade elevation exceeding 30 inches (762 mm) and 10 percent measured between an entrance and all vehicular or pedestrian arrival points within 50 feet (15 240 mm) of the planned entrance; or
2. If there are no vehicular or pedestrian arrival points within 50 feet (15 240 mm) of the planned entrance, the unusual characteristics result in a difference in finished grade elevation exceeding 30 inches (762 mm) and 10 percent measured between an entrance and the closest vehicular or pedestrian arrival point.
11B-233.3.1.2.6.5 Additional requirements. In buildings without elevators and where site impracticality test numbers one, two or three reduce the required number of residential dwelling units with adaptable features, the remaining units shall provide the following:
1. Grab bar reinforcement complying with Section 11B-809.10.5.2, 11B-809.10.6.4 or 11B-809.10.7.3.
2. Interior door opening width complying with Section 11B-404.2.3.
3. Door and gate hardware complying with Section 11B-404.2.7.
4. Door signal devices complying with Section 11B-809.8.4.
5. Door maneuvering clearance complying with Section 11B-809.8.
6. Water closet seat height complying with Section 11B-809.10.7.4.
7. Electrical receptacles, switches and controls complying with Section 11B-809.12.
8. Faucets complying with Section 11B-809.10.8.6.
9. Water closet, bathtub and lavatory maneuvering clearances complying with Section 11B-809.10.
10. Removable base cabinets complying with Section 11B-809.9.3.
Notation: 
Authority: Government Code Section 4450 and 12955.1(c)
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 18-1
Withdrawn prior to CAC.

ITEM 19-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-308.1.2 Corner Receptacle
11B-308.1 General. Reach ranges shall comply with Section 11B-308.
11B-308.1.1 Electrical switches. Controls and switches …
11B-308.1.2 Electrical receptacle outlets. …
11B-308.1.2.1. Electrical receptacles at corner work surfaces. In residential dwelling units with mobility features and residential dwelling units with adaptable features where receptacles are provided in a kitchen at a corner work surface, one receptacle shall be located 36 inches (915 mm) from either wall at the inside corner.

FIGURE 11B-308.1.2.1 - ELECTRICAL RECEPTACLES AT CORNER WORK SURFACES












Notation: 
Authority: Government Code Section 4450 and 12955.1(c)
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 20-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-403.5 Clearances
11B-403.5 Clearances.  …
Exception: Within employee work areas in facilities that are not public housing, clearances on common use circulation paths shall be permitted to be decreased by work area equipment provided that the decrease is essential to the function of the work being performed.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 21-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-805.2
11B-805.2 Patient bedrooms, and resident sleeping rooms and on-call rooms. Patient bedrooms, and resident sleeping rooms, and physician or staff on-call rooms required to provide mobility features shall comply with Section 11B-805.2.
	11B-805.2.1 Hand washing fixtures. …
	11B-805.2.2 Beds. …
	11B-805.2.3 Turning space. …
	11B-805.2.4 Toilet and bathing rooms. …
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 22-1 through 22-6
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-809.12
11B-809.12 Electrical receptacles, controls and switches. Electrical receptacles on branch circuits of 30 amperes or less, communication system receptacles, controls and switches shall be located as follows: comply with Sections 11B-308 and 11B-309.
1. Where there is no obstruction, 48 inches (1219 mm) maximum measured from the top of the receptacle box and 15 inches (381 mm) minimum measured from the bottom of the receptacle box to the finish floor.
2. Where the reach is over an obstruction, electrical receptacles, controls and switches shall comply with Sections 11B-308.3 and 11B-309.2.
3. When the reach is over a kitchen Where receptacles, controls and switches are located over a work surface and base cabinet, the work surface shall be permitted to be 36 inches (914 mm) maximum above the finish floor and 25½ inches (650 mm) maximum in depth. The base cabinet shall be 24 inches (610 mm) maximum in depth. (Relocate #3 to become Exception 5 below)
4. Where receptacles are provided in a kitchen at a corner work surface, one receptacle shall be located 36 inches (915 mm) from either wall at the inside corner.
	Exceptions:
a. 1. Electrical receptacles installed as part of in permanently installed baseboard heaters.
b. Electrical receptacles in floors adjacent to sliding panels or walls.
c. 2. Baseboard electrical receptacles in relocatable partitions, and window walls or other electrical convenience floor outlets.
d. 3. Appliances (e.g., stoves, dishwashers, range hoods, microwave ovens and similar appliances) which have controls located on the appliance.
e. Electrical receptacles dedicated to specific appliances.
f. 4. Circuit breakers.
5. (Relocate #3 from above to become Exception 5)
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Notation: 
Authority: Government Code Sections 4450 and 12955.1(c)
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 23-1
Chapter 11B Accessibility to Public Buildings, Public Accommodations, Commercial Buildings and Public Housing, Section 11B-812.4
11B-812.4 Vertical clearance. Vehicle spaces, access aisles serving them, and vehicular routes serving them shall provide a vertical clearance of 98 inches (2489 mm) minimum. Where provided, overhead cable management systems shall not obstruct required vertical clearance.
Exception: In existing multistory parking facilities, ambulatory accessible EVCS and standard accessible EVCS shall provide a vertical clearance of 80 inches (2032 mm) minimum. Existing vertical clearance in excess of 80 inches (2032 mm) and less than 98 inches (2489 mm) shall be maintained. This exception shall not apply to van accessible EVCS or vehicular routes serving them.
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 24-1 through 24-4
Chapter 35 Referenced Standards, Section ASME
ASME American Society of Mechanical Engineers …

A17.1—2019/CSA B44—19: Safety Code for Elevators and Escalators
11B-407.1, 11B-407.1.1, 11B-407.4.9, 11B-408.1, 11B-409.1, 11B-411.1, 11B-810.9, 1607.11.1, 3001.4
A17.1—13/CSA B44—2013: Safety Code for Elevators and Escalators
11B-407.1, 11B-407.1.1, 11B-407.4.9, 11B-408.1, 11B-409.1, 11B-411.1, 11B-810.9
A18.1—2020: Safety Standard for Platform Lifts and Stairway Chairlifts
1110.9, Table 3001.3
A18.1—2008: Safety Standard for Platform Lifts and Stairway Chairlifts
11B-410.1
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.

ITEM 25-1 through 25-4
Chapter 35 Referenced Standards, Section BHMA
BHMA	 Builders Hardware Manufacturers’ Association …
A 156.10—2017: Power Operated Pedestrian Doors
1010.3.2, 11B-404.2.9, 11B-404.3
A 156.10—2011: Power Operated Pedestrian Doors
11B-404.2.9, 11B-404.3
A 156.19—2019: Standard for Power Assist and Low Energy Power Operated Doors
1010.3.2, 11B-404.2.9, 11B-404.3, 11B-408.3.2.1, 11B-409.3.1
A 156.19—2013: Standard for Power Assist and Low Energy Power Operated Doors
11B-404.2.9, 11B-404.3, 11B-408.3.2.1, 11B-409.3.1
Notation: 
Authority: Government Code Section 4450
Reference(s): Government Code Section 4450 through 4452, 4456, 4457, 4459 and 12955.1. Health and Safety Code Sections 19955, 19956.5, 19957, 19958, and 19959.
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