COMMISSION ACTION MATRIX – GREEN
GREEN Building – PLUMBING, ELECTRICAL, MECHANICAL & ENERGY AD-HOC (GREEN/PEME) CODE ADVISORY COMMITTEE
2025 California mechanical code, TITLE 24, PART 4 
AGENCY: office of statewide hospital planning and development, OSHPD 05/25
LEGEND:
CAC Actions: Approve, Disapprove, Approve as Amended, Further Study Required
Agency Responses: Accept, Disagree, Withdraw 
CBSC Actions: Approve, Disapprove, Approve as Amended, Further Study Required
[bookmark: _Hlk51752204]Matrix Paper Color (for commission action only): GREEN = uncontested items, YELLOW = challenged items, SALMON = withdrawn, no action required
[bookmark: _Hlk51751202]If using assistive technology, please adjust your settings to recognize underline, strikeout, italic and ellipsis.
· Model Code language appears upright
· Existing California amendments appear in italic
· Amended model code or new California amendments appear underlined & italic
· Repealed model code language appears upright and in strikeout
· Repealed California amendments appear in italic and strikeout
· Ellipses (…) indicate existing text remains unchanged
ITEM 1
CHAPTER 3 GENERAL REGULATIONS, SECTION 320.4
OSHPD proposes to amend sections listed below.
	OSHPD 05/25
ITEM 1
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	1-1
	320.4 Telephone and Technology Equipment Centers
	Approve
	Accept
	No public comments received
	Revise OSHPD banner adding 2 & 5 and add new referenced section number.
	

	1-2
	320.4.4
	Approve
	Accept
	No public comments received
	Add text that the section does not apply to OSHPD 2 & 5.
	


ITEM 2
CHAPTER 3, SECTION 321 ESSENTIAL MECHANICAL PROVISIONS
OSHPD proposes to amend section as listed below.
	OSHPD 05/25
ITEM 2
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	2-1
	321.3
	Approve
	Accept
	No public comments received
	Add text that the section does not apply to OSHPD 3
	



ITEM 3
CHAPTER 4 VENTILATION AIR, SECTIONS 401.0, 402.0, 403.0 AND 407.0
OSHPD proposes to amend and/or add new sections listed below.
	OSHPD 05/25
ITEM 3
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	3-1
	401.1 Applicability
	Approve
	Accept
	No public comments received
	Relocate OSHPD banner and text to the end of paragraph.
	

	3-2
	402.1 Occupiable Spaces
	Approve
	Accept
	No public comments received
	Repeal OSHPD paragraph and blend into section 402.1.2 to remove duplicative and repetitive language.
	

	3-3
	402.1.2 Ventilation in Health Care Facilities
	Approve
	Accept
	No public comments received
	Blend in the paragraph from 402.1 and add reference to section 403.0 for ventilation requirements.  Add reference to the revised Table 4-C.
	

	3-4
	402.3 Mechanical Ventilation
	Approve
	Accept
	No public comments received
	Repeal OSHPD banner and text to allow pertinent information for mechanical ventilation to be used in this section.
	

	3-5
	402.4 Outdoor Air Intakes
	Approve
	Accept
	No public comments received
	Add new amendment for additional requirements for healthcare outside air intakes found in 407.2.1.
	

	3-6
	403.0 Ventilation Rates
	Approve
	Accept
	No public comments received
	Repeal OSHPD banner and text that did not permit the use for OSHPD 1, 2, 3, 4 & 5 spaces listed in Table 4-A
	

	3-7
	403.2 Zone Calculations
	Approve
	Accept
	No public comments received
	Add a reference to Table 4-A and section 407.3.1 for ventilation requirements.
	

	3-9
	407.3.1.1 Clinic Spaces
	Approve
	Accept
	No public comments received
	Add new section with requirements for ventilation systems to designed and balanced per Table 4-A or Table 4-C.
	


ITEM 4
CHAPTER 4, SECTIONS 408.0 and 415.0
OSHPD proposes to amend section as listed below.
	OSHPD 05/25
ITEM 4
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	4-1
	408.2.1
	Approve
	Accept
	No public comments received
	Add filtration level for spaces included in Table 4-A.
	

	4-2
	408.3.1
	Approve
	Accept
	No public comments received
	Add filtration level for spaces included in Table 4-A.
	

	4-3
	408.4.1
	Approve
	Accept
	No public comments received
	Add filtration level for spaces included in Tables 4-A or 4-C.
	

	4-4
	408.5.1
	Approve
	Accept
	No public comments received
	Revise reference from Table 4-B to Table 4-A.
	

	4-5
	415.1 Air Distribution
	Approve
	Accept
	No public comments received
	Add HEPA filtration for terminal device.
	


ITEM 5
CHAPTER 4, TABLE 4-A
OSHPD proposes to amend Table 4-A as listed below.
	OSHPD 05/25
ITEM 5
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	5-1
	Table 4-A – Filtration Level
	Approve
	Accept
	No public comments received
	Add filtration level column. 
	

	5-2
	Table 4-A – Post-anesthesia care unit and recovery item
	Approve
	Accept
	No public comments received
	Replace ‘NR’ with “yes” in the column for Exhausted Directly to Outdoors.
	

	5-3
	Table 4-A – Waiting area primary care clinic
	Approve
	Accept
	No public comments received
	Relocate this line item to Table 4-C.
	

	5-4
	Table 4-A – Bronchoscopy, sputum collection, and pentamidine administration
	Approve
	Accept
	No public comments received
	Revise this to “Bronchoscopy” to align with national standard.
	

	5-5
	Table 4-A – MRI room and Fluoroscopy room
	Approve
	Accept
	No public comments received
	Revise this line item for the Design Relative Humidity column from ‘NR’ to ‘MAX 60’
	

	5-6
	Table 4-A – Interventional imaging procedure room
	Approve
	Accept
	No public comments received
	Revise the required minimum outdoor air change rate from 5 ac/hr to 3 ac/hr
	

	5-7
	Table 4-A - Dental treatment
	Approve
	Accept
	No public comments received
	Relocate this line item to Table 4-C
	

	5-8
	Table 4-A – Drug room
	Approve
	Accept
	No public comments received
	Revise the space pressurization requirement to “positive”
	

	5-9
	Table 4-A – Pharmacy compounding rooms (7 rooms)
	Approve
	Accept
	No public comments received
	Replace “NR” with footnote “dd” in the Minimum Outdoor Air Change Rate column.
	

	5-10
	Table 4-A - Non-HD ante room
	Approve
	Accept
	No public comments received
	Revise air change rate from 30 ac/hr to 20 ac/hr
	

	5-11
	Table 4-A – Warewashing
	Approve
	Accept
	No public comments received
	Repeal the footnote (r).
	

	5-12
	Table 4-A – Sterilizing equipment room
	Approve
	Accept
	No public comments received
	Revise the recirculated room unit requirement from “No” to “NR”.
	

	5-13
	Table 4-A – BEHAVIORAL HEALTH
	Approve
	Accept
	No public comments received
	Add 3 space functions to be listed under new section for Behavioral Health.
Post CAC: HCAI added underline to temperature values
	

	5-14
	Table 4-A – Skilled Nursing and Intermediate Care Facilities: AII room & AII anteroom 
	Approve
	Accept
	No public comments received
	Revise footnote ‘b’ to footnote ‘u’.
	

	5-15
	Table 4-A – Resident Corridor (1225.5.1.1)
	Approve
	Accept
	No public comments received
	Revise referenced section number to 1225.5.1.1.
	

	5-16
	Table 4-A – Footnote b
	Approve
	Disagree
	No public comments received
	Revise referenced section to Board of Pharmacy requirements found in Title 16.
Post CAC: HCAI corrected Title 16 Section numbers.
	

	5-17
	Table 4-A – Footnote r
	Approve
	Accept
	No public comments received
	Replace model language with text regarding the newly added filtration level and direct code user to Table 4-B.
	

	5-18
	Table 4-A – Footnote dd
	Approve
	Accept
	No public comments received
	Revise footnote to direct code user to Section 403 to calculate the required outside air change rate.
	


ITEM 6
CHAPTER 4, TABLE 4-B
[bookmark: _Hlk217026346]OSHPD proposes to amend Table 4-B as listed below.
	OSHPD 05/25
ITEM 6
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	6-1
	Table 4-B
	Approve
	Accept
	No public comments received
	Consolidate Table 4-B to include requirements of Table 4-B and 4-C with further amendments. Amend the title of the table to include skilled nursing facilities, intermediate care facilities, and correction treatment centers adding OSHPD 2 & 4 to the banner.
	

	6-2
	Table 4-B – Filtration Level
	Approve
	Accept
	No public comments received
	Add new column for ‘Filtration Level’.  
	


ITEM 7
CHAPTER 4, TABLE 4-C
OSHPD proposes to amend Table 4-C as listed below.
	OSHPD 05/25
ITEM 7
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	7-1
	Table 4-C FILTER EFFICIENCIES FOR CENTRAL VENTILATION … [OSHPD 2 & 4]
	Approve
	Accept
	No public comments received
	Repeal Table 4-C about filter efficiencies and relocate the requirements of Table 4-C to Table 4-B.  
	

	7-2
	Table 4-C PRESSURE RELATIONSHIP & VENTILATION REQUIREMENTS FOR LICENSED CLINICS [OSHPD 3] 
	Approve
	Accept
	No public comments received
	Add new Table 4-C related to ventilation requirements for certain licensed clinics. This table is based on Table 8-2 from the 2021 ASHRAE 170 Standard with further OSHPD amendments.
	

	7-3
	Table 4-C Footnote a
	Approve
	Accept
	No public comments received
	Revise footnote a to reference appropriate California Mechanical Code (CMC) Section 407.4.5
	

	7-4
	Table 4-C Footnote b
	Approve
	Accept
	No public comments received
	Revise footnote b to clarify functions not specifically addressed in Table 8-2.
	

	7-5
	Table 4-C Footnote c
	Approve
	Accept
	No public comments received
	Revise footnote c to refer to Table 4-B.
	

	7-6
	Table 4-C Footnote d
	Approve
	Accept
	No public comments received
	Revise footnote d to match amendment in Table 4-A
	

	7-7
	Table 4-C Footnote f
	Approve
	Accept
	No public comments received
	Revise references for the Facility Guidelines Institute to the appropriate California Building Code (CBC) Section.
	

	7-8
	Table 4-C Footnote g
	Approve
	Accept
	No public comments received
	Revise to match the primary care clinic waiting room function of space.  Note clarifies the room function is intended for primary care clinics and other clinic types.
	

	7-9
	Table 4-C Footnote j
	Approve
	Accept
	No public comments received
	Replace model language with amended language from Table 4-A related to exhaust. 
	

	7-10
	Table 4-C Footnotes l & m & p
	Approve
	Accept
	No public comments received
	Revise references from Tables 7-1 / 8-1 to Table 4-A.
	

	7-11
	Table 4-C Footnotes n & o
	Approve
	Accept
	No public comments received
	Revise references from Table 8-1 to Table 4-A and modify to match the CBC Section 1224.
	

	7-12
	Table 4-C Footnote q
	Approve
	Accept
	No public comments received
	Replace model language with requirements of Section 403 for ventilation systems using air class design option.
	

	7-13
	Table 4-C Footnote r
	Approve
	Accept
	No public comments received
	Add new footnote for toilet exhaust requirements.
	


ITEM 8
CHAPTER 5 EXHAUST SYSTEMS, SECTION 505.0 PRODUCT-CONVEYING SYSTEMS 
OSHPD proposes to amend sections listed below.
	OSHPD 05/25
ITEM 8
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	8-1
	507.7 505.13 Pharmaceutical Hazardous Drug (HD) Compounding Exhaust Discharge
	Approve
	Accept
	No public comments received
	Relocate this section and add ‘hazardous drug’ to identify that the requirements apply to hazardous exhaust. Revise discharge height from 7 to 10 feet to align with Section 407.2.2.1.
	




ITEM 9
CHAPTER 6 DUCT SYSTEMS, SECTION 602.0 MATERIAL
OSHPD proposes to amend section listed below.
	OSHPD 05/25
ITEM 9
	Code Section
	CAC
Action
	Agency Response
	Public Comments
	Annotations
	CBSC
Action

	9-1
	602.1 General
	Approve
	Disagree
	No public comments received
	Relocate OSHPD banner to the end of the exception and remove banner [Not permitted for OSHPD 1, 1R, 2, 3, 4 & 5] which is no longer needed.
Post CAC: HCAI revised referenced section from 407.4.2 to 407.4.3.
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