STATE OF CALIFORNIA
BUILDING STANDARDS COMMISSION

Agenda Item 2c – Supplement for Section 5.106.5.4 #2
5.106.5.3.2.4. Electric vehicle charging stations (EVCS). EV capable spaces shall be provided with electric vehicle supply equipment (EVSE) to create EVCS in the number indicated in Table 5.106.5.3.1. The EVCS required by Table 5.106.5.3.1 shall be provided with Level 2 EVSE or DCFC as permitted in Section 5.106.5.3.2.3. At least one Level 2 EVSE shall be provided. When EVCS are provided, they shall comply with the following requirements: 
1. Multiple connectors. One EV charger with multiple connectors …
OPTION 1:
5.106.5.3.2.2 EV charger connectors. EV chargers shall be equipped with SAE J1772 with a maximum output 240 Volts AC or SAE J3400 connectors.
When using level 2 SAE J3400 SAE connectors, supplied by a 480 V 3-phase service, at least 20 percent of the EV charger connectors shall be SAE J1772 with a maximum output 240 Volts AC. 
RATIONALE: 
In Option 1, it is proposed to repeal all the requirements specifying allowed connector types. The BSC intent of the CALGreen Code is not to prohibit any EV connector types or emerging EV charging technologies.

OPTION #2:
2. 5.106.5.3.2.2 EV charger connectors. EV chargers shall be compatible equipped with one of the following connectors: 
a. SAE J1772 with a maximum output of 240 Volts AC. or 
b. SAE J3400. connectors 
c. SAE J3068. 
When using SAE J3068 connectors, the connectors shall be allowed to provide a socket-outlet for a detachable charging cable assembly in lieu of an attached cable. 
When using level 2 SAE J3400 connectors, supplied by a 480 V 3-phase service, at least 20 percent of the EV charger connectors shall be SAE J1772 with a maximum output 240 Volts AC.
RATIONALE: 
In Option 2, as requested during the first CALGreen workshop, SAE J3068 connectors are proposed to be added to the code section as an allowed connector. Also, language is proposed to clarify that J3068 connectors are allowed to provide a socket-outlet for a detachable charging cable assembly in lieu of an attached cable.
Additionally, existing language requiring 20% of the connectors to be SAE J1772 in certain circumstances is proposed to be revised to remove possible conflicts with level 2 EVSE definition. 
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