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DRAFT EXPRESS TERMS 
AGENDA ITEM 3a
Chapter 5 NONRESIDENTIAL MANDATORY MEASURES
Division 5.1 – PLANNING AND DESIGN
SECTION 5.106 – SITE DEVELOPMENT
5.106.4 Bicycle parking. For buildings within the authority of California Building Standards Commission as specified in Section 103, comply with Section 5.106.4.1. For buildings within the authority of the Division of the State Architect pursuant to Section 105, comply with Section 5.106.4.2. Bicycle parking for buildings within the authority of the California Building Standards Commission (BSC-CG), as specified in Section 103, shall comply with Section 5.106.4.1. Bicycle parking for buildings within the authority of the Division of the State Architect (DSA-SS), as specified in Section 105, shall comply with Section 5.106.4.2.
5.106.4.1 Bicycle parking for buildings within BSC-CG authority. [BSC-CG] Comply Bicycle parking shall be provided in accordance with Sections 5.106.4.1.1 and 5.106.4.1.2 Section 5.106.4.1.1, 5.106.4.1.2 or 5.106.4.1.3; or shall meet the an applicable local ordinance, whichever is stricter. Calculations for bicycle parking requirements shall be rounded up to the nearest whole number.
Short-term bicycle parking shall comply with Section 5.106.4.1.4. Long-term bicycle parking shall comply with Section 5.106.4.1.5.
Exceptions: 
At the enforcing authority's discretion, bicycle parking shall be permitted to be reduced or eliminated for projects in buildings where any of the following apply:
1. Projects that do not have physical space to accommodate bicycle parking.
1. Travel by bicycle to the site is impossible or infeasible.
1. Equivalent bicycle parking of equal quantity is provided within the envelope of the building.
1. Number of required combined short and long-term bicycle parking spaces exceeds 50.
1. Free valet bicycle parking is provided.
5.106.4.1.1 New buildings. New buildings shall be provided with short-term bicycle parking for 3 percent of the total occupant load with a minimum of one two-bike capacity rack and long-term bicycle parking for 1 percent of the total occupant load. 
5.106.4.1.2 Additions and alterations. Additions and alterations to existing buildings shall be provided with short-term bicycle parking for 3 percent of the added occupant load with a minimum of one two-bike capacity rack and long-term bicycle parking for 1 percent of the added occupant load.
5.106.4.1.3 New shell buildings. New shell buildings in phased projects shall be provided with short-term bicycle parking for 3 percent of the anticipated occupant load with a minimum of one two-bike capacity rack and long-term bicycle parking for 1 percent of the anticipated occupant load.
5.106.4.1.1 5.106.4.1.4 Short-term bicycle parking. If the new project or an addition or alteration is anticipated to generate visitors, provide permanently anchored bicycle racks within 200 feet of the visitors’ entrance, readily visible to passers-by, for 20 percent of the peak daily visitors, with a minimum of one two-bike capacity rack. Acceptable short-term bicycle racks shall be permanently anchored, shall be visible from the building entrance, and shall be installed no greater than 200 feet from the primary entrance to the building. Where buildings are served by more than one primary entrance, the quantity of racks shall be distributed near both entrances for the convenience of the users.
5.106.4.1.2 5.106.4.1.5 Long-term bicycle parking. Acceptable long-term bicycle parking facility for Sections 5.106.4.1.2.1, 5.106.4.1.2.2 and 5.106.4.1.2.3 shall be conveniently located near the street or building entrance and shall meet one of the following:
1. Covered, lockable enclosures with permanently anchored racks for bicycles;
2. Lockable bicycle rooms with permanently anchored racks; or
3. Lockable, permanently anchored bicycle lockers.
5.106.4.1.2.1 For new buildings with tenant spaces, provide secure bicycle parking for 10 percent of the tenant-occupants, with a minimum of one bicycle parking facility.
5.106.4.1.2.2 For additions or alterations, provide secure bicycle parking for 10 percent of the tenant-occupants being added, with a minimum of one bicycle parking facility.
5.106.4.1.2.3 For new shell buildings in phased projects, provide secure bicycle parking for 10 percent of the anticipated tenant-occupants, with a minimum of one bicycle parking facility.
RATIONALE:
BSC-CG is proposing amendments in Section 5.106.4 about bicycle parking for buildings withing BSC-CG authority and related sub-sections.
BSC-CG received feedback from code users and the regulated community which have expressed concerns with the use of “peak daily visitors” or “tenant-occupants” as the basis for determining quantity requirements for short-term and long-term bicycle parking. These terms have proved to be hard to determine and enforce. BSC-CG has also received comments that the recent change in bike parking requirements that happened in the 2025 CALGreen during the 2024 triennial code adoption cycle resulted in excessive number of required bicycle parking spaces. These excessive bike parking requirements are causing existing vehicular parking spaces to be converted into bike parking, which can be burdensome, and there are projects that may not have physical space to accommodate the bicycle parking. The proposed amendments are intended to address these issues.
BSC-CG researched international code language (2024 International Green Construction Code (IGCC) developed by the International Code Council) and several local ordinances addressing this topic and found that they base bike parking quantities on occupant load, number of vehicle parking spaces or other methods. BSC-CG has decided to base the regulations in CALGreen Code on Occupant Load as it is a widely used defined term in the California Building Code (Part 2 of Title 24 Code of Regulations) and is easily quantifiable, thus providing a finite, defined method for calculating the requirements for compliance.
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BSC-CG created three “sample projects” and calculated the required number of short-term and long-term bicycle parking spaces based on select local jurisdictions, the 2024 IGCC, and the 2022 edition of CALGreen Code, as well as the proposed amendments for the 2027 Code Adoption Cycle. The proposed values were set with the intent of not decreasing or increasing the values required in the 2022 CALGreen. Additionally, exceptions are proposed to be included to address “outlier” projects, as the discretion of the local Authority Having Jurisdiction.
	 CALGreen CEVW Workshop #2 (10-29-2026)

Breakdown of requirements for select local ordinances and State & International Codes
	Jurisdiction
	Short term
	Long term
	Method of Calculation

	City of Davis
	< 2 hours parking (Visitors, customers)
	>2 hours parking (Residents, employees)
	1 per <SF> based on use

	Office
	75% short-term
	25 % long term
	1 per 1,500 SF

	Industrial
	25% short-term
	75% short-term
	1 per 7,500 SF

	Restaurant (Sit-down)
	75% short-term
	25 % long term
	1 per 500 SF

	City of Citrus Heights
	1 per 20 veh. spaces (Up to 100, retail and office)
	N/A
	per vehicle space

	City of Roseville
	10% of vehicle spaces
	N/A
	per vehicle space

	City of San Francisco
	Class 2'. Varies (Min. 5% of veh. parking)
	Class 1'. Varies (Min. 5% of veh. parking)
	Per "occupied SF"; based on use

	Industrial
	4 for spaces > 50k SF
	1 per 12k SF; Min. 2
	

	Eating & Drinking Uses (Restaurant)
	1 per 750 SF; Min. 2
	1 per 7,500 SF
	

	Office
	2 for > 5k SF
	1 per 5k sf
	

	City of Los Angeles
	
	
	Per SF (Min. per 2)

	Office
	1 per 10k sf
	1 per 5k sf
	1 per 'x' SF

	Warehouse
	1 per 10k sf
	1 per 10k sf
	1 per 'x' SF

	Restaurants & Bars
	2 per restaurant
	2 per restaurant
	 

	Based on comparing with 2022 CALGreen
	5% / New Visitor Vehicle parking
	5% / Tenant-occupant parking
	% of vehicle parking

	Proposed CALGreen values
	3% of occ. Load
	1% of occ. Load
	% of occ. Load

	IGCC by ICC values
	5% of occ. Load
	N/A
	% of occ. Load


Note: For local jurisdictions that use “Uses”, all uses provided by the jurisdiction are not necessarily listed in this table.
	Jurisdiction
	10k SF office (150sf/occ)
	Sample 2k SF restaurant (15sf/occ)
	Sample 80,000 SF warehouse (300sf/occ)

	Assumed Occupants
	67
	134
	267

	City of Davis
	
	
	

	Office
	7 Total (5 short /2 long)
	 -
	 -

	Industrial
	 -
	 -
	11 Total (3 short / 8 long)

	Restaurant (Sit-down)
	 
	4 Total (3 short / 1 long)
	 

	City of Citrus Heights
	2 short
	1 short
	4 short

	City of Roseville
	3 short
	2 short
	8 short

	City of San Francisco
	 
	 
	 

	Industrial
	 
	 
	4 short / 7 long

	Eating & Drinking Uses (Restaurant)
	 
	3 short / 4 long
	 

	Office
	2 short / 2 long
	 
	 

	City of Los Angeles
	 
	 
	 

	Office
	1 short / 2 long
	 
	 

	Warehouse
	 
	 
	8 short / 8 long

	Restaurants & Bars
	 
	2 short / 2 long
	 

	Based on comparing with 2022 CALGreen
	4 short
	7 short
	8 short

	Proposed CALGreen values
	1 short / 1 long
	2 short / 1 long
	8 short / 8 long

	IGCC by ICC values
	3 short / 2 long
	4 short / 2 long
	4 short / 4 long


Sample Projects



















Note: Assumed occupant load for sample projects do not consider ancillary or accessory occupancy space.



