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[bookmark: _Hlk200621048]The state agency shall draft the regulations in plain, straightforward language, avoiding technical terms as much as possible and using a coherent and easily readable style. The agency shall draft the regulation in plain English. A notation shall follow the express terms of each regulation listing the specific statutes authorizing the adoption and listing specific statutes being implemented, interpreted, or made specific (Government Code Section 11346.2(a)(1)).
[bookmark: _Hlk110847738]If using assistive technology, please adjust your settings to recognize underline, strikeout and ellipsis.

LEGEND for EXPRESS TERMS 
· Existing California language appears upright.
· Proposed amendments appear in underline and strikeout.
· Ellipses ( ...) indicate existing text remains unchanged.
· [bookmark: _Hlk200620172]Rationale: The justification for the change is shown after each section or series of related changes.
[bookmark: _Hlk200620384]
DRAFT EXPRESS TERMS 
AGENDA ITEM 3g
APPENDIX A5 NONRESIDENTIAL VOLUNTARY MEASURES,
DIVISION A5.1 – PLANNING AND DESIGN,
SECTION A5.106 SITE DEVELOPMENT
[bookmark: _Hlk199329276]A5.106.4 Reserved. Bicycle accommodation electives. 
[Section A5.106.4.1 – Option 1]
A5.106.4.1 Reserved. Electric bicycle (E-bike) charging. For buildings with long-term bicycle parking facilities required per Section 5.106.4.1, one e-bike charging receptacle with a minimum 20A duplex 120V AC power supply outlet shall be provided. The receptacle shall be installed within the locations listed in Section 5.106.4.1.5. Proprietary equipment for e-bike charging can be used, provided the equipment will universally charge commercially available e-bikes. Electrical equipment shall be installed in compliance with the California Electrical Code. E-bike charging areas shall comply with California Fire Code.
[Section A5.106.4.1 – Option 2]
A5.106.4.1 Reserved. Electric bicycle (E-bike) charging. For buildings with long-term bicycle parking facilities required per Section 5.106.4.1, one e-bike charging 20A/120V receptacle outlet shall be provided per 5 long-term bicycle parking spaces. The receptacle shall be installed within the locations listed in Section 5.106.4.1.5. Proprietary equipment for e-bike charging can be used, provided the equipment will universally charge commercially available e-bikes. Electrical equipment shall be installed in compliance with the California Electrical Code. E-bike charging areas shall comply with California Fire Code.
Exception: A duplex receptacle shall be considered two individual receptacles.
A5.106.4.2 Reserved. A5.106.4.3 Changing rooms. For buildings with 3 or more long-term bicycle parking spaces over 10 tenant-occupants, provide changing/shower facilities shall be provided for tenant-occupants long-term bicycle parking space users only in accordance with Table A5.106.4.32 or document arrangements with nearby changing/shower facilities.
Exception: Shared shower facilities existing within the building may be utilized to satisfy the requirements of this section, provided the aggregate fixture count complies with the provisions of this section. Such facilities shall, at a minimum, include one unisex shower and two 2-tier lockers.
Note: Additional information on recommended bicycle accommodations may be obtained from Sacramento Area Bicycle Advocates at https://sacbike.org.
TABLE A5.106.4.32
	NUMBER OF LONG-TERM BICYCLE PARKING SPACES TENANT-OCCUPANTS
	SHOWER/CHANGING 
FACILITIES REQUIRED 2
	2-TIER (12" X 15" X 72") PERSONAL EFFECTS LOCKERS1, 2 REQUIRED

	0-10 1-2
	0
	0

	11-50 3-6
	1 unisex shower
	2

	101-200 7-9
	1 shower stall per gender
	4

	Over 200 10
	1 shower stall per gender for each 200 10 additional tenant-occupants long-term bicycle parking spaces
	Two One 2-tier lockers for each 50 additional tenant-occupants shower stall.



1. One 2-tier locker serves two people. Lockers shall be lockable with either padlock or combination lock.
2. Tenant spaces housing more than 10 tenant-occupants within buildings sharing common toilet facilities need not comply; however, such common shower facilities shall accommodate the total number of tenant-occupants served by the toilets and include a minimum of one unisex shower and two 2-tier lockers.
RATIONALE: 
BSC-CG is proposing to amend voluntary regulations for changing rooms, add new voluntary regulations for E-bike charging, and clarify that these regulations are electives related to bicycle accommodation. 
E-Bike charging
New voluntary E-Bike charging regulations are proposed in response to the comments received during the 2024 Code Adoption Cycle 45-day public comment period. BSC staff received public comments from the California Bicycle Coalition, which represents over 60,000 members, and various individuals and organizations stating the need for E-Bike charging for long-term bicycle parking.
During the first CEVW Workshop, a comment was made about using a duplex outlet versus a single outlet due to potential of tripping the circuit breaker if two fast charger e-bikes, which can pull up to 6 amps each, are charged simultaneously at the same duplex outlet. BSC-CG researched the possible issues raised by the commenter, revised the regulations and is seeking public input on the two options with proposed language. Most 120V receptacles used for charging will require ground-fault circuit-interrupter (GFCI) protection. However, GFCI protects the user from electrical shock, not from overloading the outlet or overheating, so considering the evolving technology and appearance of the fast-charging bikes, limiting the number of the outlets in one receptacle or specifying minimum amperage of 20A may provide additional safety. 
Changing rooms
BSC-CG is proposing to amend the language of the changing room elective to base the requirements on the number of long-term bicycle parking spaces rather than “tenant-occupants” to align with changes made in mandatory section requirements for bicycle parking. The number of long-term bicycle parking spaces is determined in Section 5.106.4.1. Table A5.106.4.2 provides incrementally increasing requirements for shower facilities to accommodate occupants who elect to commute by bicycle. The proposal is intended to be non-regulatory to require the same number of shower stalls and lockers as is required by the current regulations. To formulate equivalent quantities for the requirements, a sample project of 10,000 SF was assumed and used to indicate the resulting percentages used in the provisions. Additionally, TABLE A5.106.4.2 footnote 2 is proposed to be repealed and its content editorially revised and proposed as an exception.
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