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DRAFT EXPRESS TERMS 
AGENDA ITEM 3k
CHAPTER 5 NONRESIDENTIAL MANDATORY MEASURES,
DIVISION 5.4 – MATERIAL CONSERVATION AND RESOURCE EFFECIENCY,
SECTION 5.407 WATER RESISTENCE AND MOISTURE MANAGEMENT 
…
5.407.2 Moisture control. …
5.407.2.1 Sprinklers. …
5.407.2.2 Entries and openings. Design exterior entries and/or openings subject to foot traffic or wind-driven rain to prevent water intrusion into buildings as follows:
5.407.2.2.1 Exterior door protection. Primary exterior entries shall be covered to prevent water intrusion by using nonabsorbent floor and wall finishes within at least 2 feet around and perpendicular to such openings plus at least one of the following:
1. An installed awning at least 4 feet in depth and extending at least 1 foot horizontally beyond each side of the door opening.
2. The door is protected by a roof overhang at least 4 feet in depth.
3. The door is recessed at least 4 feet.
4. Other methods which provide equivalent protection.
5.407.2.2.2 Flashing. …
RATIONALE: 
BSC-CG is proposing amendments in the existing section 5.407.2.2.1 about exterior door protections. This code proposal was added post 1st CALGreen workshop conducted on September 1, 2026, and is being co-adopted with DSA. 
BSC-CG proposes removing the requirement for nonabsorbent wall finishes at exterior entries. The moisture concerns associated with these conditions relate primarily to the floor surfaces, where water can be tracked in on shoes and absorbed. Because wall finishes do not contribute to moisture retention in this scenario, maintaining the requirement for nonabsorbent floor finishes alone is adequate to meet the intent of the section.
BSC CG also proposes to require awnings used for compliance with the section to extend a minimum of one foot horizontally beyond both sides of the door opening. This added lateral coverage is necessary to better protect against wind driven rain, which can reach the sides of the door even with sufficient overhead depth. Extending the awning helps prevent water intrusion at the door.
Cost TBD. BSC and DSA staff are working on obtaining the cost data associated with this proposal.
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