INITIAL EXPRESS TERMS  
FOR PROPOSED BUILDING STANDARDS  
OF THE **DIVISION OF THE STATE ARCHITECT (DSA-SS AND DSA-SS/CC)**  
REGARDING THE **2019 CALIFORNIA PLUMBING CODE**,  
CALIFORNIA CODE OF REGULATIONS, TITLE 24, PART **5**

# (DSA-SS/CC XX/19)

The State agency shall draft the regulations in plain, straightforward language, avoiding technical terms as much as possible and using a coherent and easily readable style. The agency shall draft the regulation in plain English. A notation shall follow the express terms of each regulation listing the specific statutes authorizing the adoption and listing specific statutes being implemented, interpreted, or made specific (Government Code Section 11346.2(a)(1)).

Note: Select the appropriate legend below and delete the legend that is not used.

If using assistive technology, please adjust your settings to recognize underline, strikeout, italic and ellipsis.  
**LEGEND FOR EXPRESS TERMS (Based on model codes - Parts 2, 3, 4, 5, 10)**

1. Model Code language appears upright.
2. Existing California amendments appear in *italics*.
3. Amended model code or new California amendments appear *underlined and in italics*.
4. Repealed model code language appears ~~upright and in strikeout~~.
5. Repealed California amendments appear in *~~italics~~* ~~and~~ *~~strikeout~~*.
6. Ellipsis indicates existing text remains unchanged.

If using assistive technology, please adjust your settings to recognize underline, strikeout and ellipsis.  
**LEGEND FOR EXPRESS TERMS (California only codes - Parts 1, 8, 11, 12)**

1. Existing California amendments appear upright.
2. Amended or new California amendments appear underlined.
3. Repealed California language appears ~~upright and in strikeout~~.
4. Ellipsis indicates existing text remains unchanged.

## INITIAL EXPRESS TERMS

**ITEM 1: PRE-RINSE SPRAY VALVES**

**SECTION 5.303**

**INDOOR WATER USE**

**. . .**

**5.303.3.4.5 Metering faucets for wash fountains.** Metering faucets **. . .**

**Note:** Where complying faucets **. . .**

**. . .**

**5.303.3.4.6 Pre-rinse spray valve.** When installed, shall meet the requirements in the California Code of Regulations, Title 20 (Appliance Efficiency Regulations), Section 1605.1 (h)(4) Table H-2, Section 1605.3 (h)(4)(A), *Section 1607(d)(7,) and* equipped with an integral automatic shutoff.

FOR REFERENCE ONLY: The following table and code section has been reprinted from the Title 20 (Appliance Efficiency Regulations), Section 1605.1 (h)(4) and Section1605.3 (h)(4)(A)

Table H-2

Standards for Commercial Pre-rinse Spray Valves Manufactured on

or After January 28, 2019

| **Product Class (spray force in ounce force (ozf))** | **Maximum Flow Rate (gpm)** |
| --- | --- |
| Product Class 1 (≤ 5.0 ozf) | 1.0 |
| Product Class 2 (> 5.0 ozf and ≤ 8.0 ozf) | 1.20 |
| Product Class 3 (> 8.0 ozf) | 1.28 |

Title 20 Section 1605.3(h)(4)(A): Commercial pre-rinse spray valves manufactured on or after January 1, 2006, shall have a minimum spray force of not less than 4.0 ounces-force (ozf) [113 grams-force (gf)]

**. . .**

**Notation for [DSA-SS]**

**Authority:** Education Code Sections 17310 and 81142, and Health and Safety Code Section 16022.

**Reference:** Education Code Sections 17280 through 17317, 81130 through 81147 and Health and Safety Code Sections 16000 through 16023.

**Notation for [DSA-SS/CC]**

**Authority:** Education Code Section 81053.

**Reference:** Education Code Sections 81052, 81053, and 81130 through 81147.