# ADDITIONAL 15-DAY EXPRESS TERMS AND RATIONALEFOR PROPOSED BUILDING STANDARDSOF THE DIVISION OF THE STATE ARCHITECT

# (DSA-SS and DSA-SS/CC)REGARDING THE 2022 CALIFORNIA PLUMBING CODE,

# CALIFORNIA CODE OF REGULATIONS, TITLE 24, PART 5

# (DSA SS/CC 02/21)

No state agency may adopt, amend, or repeal a regulation which has been changed from that which was originally made available to the public pursuant to Section 11346.5, unless the change is (1) nonsubstantial or solely grammatical in nature, or (2) sufficiently related to the original text that the public was adequately placed on notice that the change could result from the originally proposed regulatory action. If a sufficiently related change is made, the full text of the resulting adoption, amendment, or repeal, with the change clearly indicated, shall be made available to the public for at least 15 or 45 days before the agency adopts, amends, or repeals the resulting regulation.

Any written comments received regarding the change must be responded to in the final statement of reasons required by Section 11346.9 (Government Code Section 11346.8(c)).

If using assistive technology, please adjust your settings to recognize underline, strikeout, double strikeout, italics and ellipsis. Double underline will be indicated by parenthetical notes within the text. The notes will not be codified or published in the code.

## LEGEND for EXPRESS TERMS (Based on model codes - Parts 2, 2.5, 3, 4, 5, 9, 10)

* Model Code language appears upright.
* Unmodified California 45-day amendments appear in *underline and italic* and *~~strikeout and italic~~.*
* California additional 15-day amendments appear in *double underline and italic* and *double strikeout and italic*.
* Ellipsis ( ...) indicate existing text remains unchanged.
* **Rationale**: The justification for the change is shown after each section or series of related changes.

# ADDITIONAL 15-DAY EXPRESS TERMS

# Item 4

# Chapter 4, Plumbing fixtures and fixture fittings

DSA proposes to adopt Chapter 4 of the 2021 UPC into the 2022 edition of the CPC with existing California amendments carried forward and additional changes.

…

**422.1 Fixture Count.** Plumbing fixtures shall be provided for the type of building occupancy and in the minimum number shown in Table 422.1 ***[OSHPD 1,1R,2,3,4 & 5]*** *and Tables 4-2 and Table 4-3.* The total occupant load and occupancy classification shall be determined in accordance with the *California Building Code* ***[******DSA-SS & DSA-SS/CC]*** *or Occupant Load Factor Table A.* Occupancy classification not shown in Table 422.1 shall be considered separately by the Authority Having Jurisdiction.

*[begin double underline]* ***Exception:*** *[end double underline]* ***[BSC,*** *[begin double underline]* ***DSA-SS & DSA-SS/CC]*** *Using occupancy classification, described as function of space, determine occupant load factor from Table 4-1 Occupant Load Factor, of this chapter.* *[end double underline]*

…

**Rationale:** DSA originally intended to co-adopt BSC amendments to CPC Section 422.1, language at the top of Table 422.1, and Table 4-1. However, co-adopted amendments to Section 422.1 referenced in the ISOR were inadvertently omitted from DSA’s 45-day express terms and are included herein for 15-day public comment. These proposed changes align with sufficiently-related changes DSA is proposing to CPC Tables 422.1 and 4-1, in coordination with BSC.

**Notation: DSA-SS**

Authority: Education Code Sections 17310 and 81142, and Health and Safety Code Section 16022.

Reference(s): Education Code Sections 17280 through 17317, and 81130 through 81147, and Health and Safety Code Sections 16000 through 16023.

**Notation: DSA-SS/CC**

Authority: Education Code Section 81053.

Reference(s): Education Code Sections 81052, 81053, and 81130 through 81147.