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[bookmark: _Hlk199329276]A5.106.4 Reserved. Bicycle accommodation electives. Provide electric bicycle (e-bike) charging in accordance with Section A5.106.4.1. 
A5.106.4.1 Reserved. Electric bicycle (E-bike) charging. E-bike charging shall comply with Section A5.106.4.1.1.
A5.106.4.1.1 Long-term electric e-bike charging. Where long-term bicycle parking facilities are provided per mandatory Sections 5.106.4.1.2 through 5.106.4.1.2.3, provide one e-bike charging receptacle with a minimum of (2) outlets with 120V AC power supply. Install receptacle within the locations listed in mandatory Section 5.106.4.1.2. Electrical equipment or receptacle shall be installed in compliance with the California Electrical Code.
A5.106.4.3 2 Changing rooms elective. For buildings with 3 or more long-term bicycle parking spaces over 10 tenant-occupants, provide changing/shower facilities for tenant-occupants long-term bicycle parking space users only in accordance with Table A5.106.4.3 or document arrangements with nearby changing/shower facilities.
Note: Additional information on recommended bicycle accommodations may be obtained from Sacramento Area Bicycle Advocates at https://sacbike.org.


	TABLE A5.106.4.3

	NUMBER OF LONG-TERM BICYCLE PARKING SPACES TENANT-OCCUPANTS
	SHOWER/CHANGING FACILITIES REQUIRED 2
	2-TIER (12" X 15" X 72") PERSONAL EFFECTS LOCKERS1, 2 REQUIRED

	0-10 1-2
	0
	0

	11-50 3-6
	1 unisex shower
	2

	101-200 7-9
	1 shower stall per gender
	4

	Over 200 10
	1 shower stall per gender for each 200 additional tenant-occupants 10 long-term bicycle parking spaces.
	One 2-tier locker
for each 50 10 additional tenant-occupants

	1. One 2-tier locker serves two people. Lockers shall be lockable with either padlock or combination lock.
2. Tenant sSpaces housing more than 200 tenant-occupants 10 long-term bicycle spaces within buildings sharing common toilet facilities need not comply; however, such common shower facilities shall accommodate the total number of tenant-occupants long-term bicycle parking space users served by the toilets and include a minimum of one unisex shower and two 2-tier lockers.


RATIONALE: 
BSC-CG is proposing to amend Section A5.106.4 by adding new voluntary code language for E-bike charging. This language is proposed in response to the comments received during the 2024 Code Adoption Cycle 45-day public comment period. BSC staff received public comments from the California Bicycle Coalition, which represents over 60,000 members, and various individuals and organizations stating the need for E-Bike charging for long-term bicycle parking.
Additionally, BSC-CG is proposing to amend the language of the changing room elective to base the requirements on the number of long-term bicycle parking spaces rather than “tenant-occupants”. The number of long-term bicycle parking spaces is determined in Section 5.106.4.1.2. Table A5.106.4.3 provides incrementally increasing requirements for facilities to accommodate occupants who elect to commute by bicycle.
Lastly, BSC-CG is amending the title to Section A5.106.4.3 2 Changing rooms to add the word elective to clearly identify that changing rooms is to be considered a separate elective measure. 
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